# HolbyMonitor Quick Start Instructions

# Setup Base Station

* Attach wireless antenna
* Plug in Ethernet cable
* Plug in AC Power Adapter

# Setup Node

* Remove battery panel
* Install 2 “D” batteries (provided), then replace battery panel
* Plug in three sensors where indicated on front of node (Blue to Cold, Black to Mix, Red to Hot)

# Install Node

* Attach Node to wall or the Cold water supply pipe near the Holby Tempering valve
* Attach the BLUE sensor to the COLD water supply pipe with a hose clamp
* Attach the BLACK sensor to the MIXED (Tempered) water pipe with a hose clamp
* Attach the RED sensor to the HOT water supply pipe with a hose clamp
* **NOTE**: ALL SENSORS MUST BE IN DIRECT CONTACT WITH THE COPPER PIPES
* Press the white Force Update button on front of node to send update to base station

# Download Free App

* Go to Apple App Store or Google Play Store on your smartphone
* Search for **HolbyMonitor**
* Download the free App to your phone
* Create a HolbyMonitor Account
* After downloading the free app, select **Create one for free!**
* Complete the Primary User information using the HolbyMonitor App or monitor.holby.com website
* Provide all required information
* Follow instructions to validate your new account

# Register Devices to Your HolbyMonitor Account

* Select **Add** **Device** to register base station to account
* Select **Add** **Device** to register node to account

# Add Contacts via HolbyMonitor App

* Select the **Menu** symbol (upper right corner)
* Select **ACCOUNT** **MANAGEMENT**, **Additional Contacts**, then **Add Contact**
* Enter required details, select **Save**